
**Press Release** **icotek KEL-DPZ-CLICK (1345/1596 digits)**

**New Cable Entry Plate KEL-DPZ-CLICK from icotek**

**KEL-DPZ-CLICK with Double Mounting Option**

With the new KEL-DPZ-CLICK up to 78 cables can be fed through just one cutout. The new cable entry plate has two different mounting options!  
The KEL-DPZ-CLICK is available for the standard metric cutouts M25, M32, M40, M50 and M63. Depending on the selected version, up to 78 cables can be routed through one cutout and thus offers an extremely space-saving and compact cable pass-through. The type of installation is left to the user and can be adapted to the situation during the installation process. The mounting options available are either by fixing it with a counter nut (wall thickness up to 11 mm) or by snapping it in (wall thickness 1 - 2.5 mm).  
With the compact, flat and hybrid KEL-DPZ-CLICK products, cables in control cabinet housings, systems and machines can be routed without plugs and sealed up to IP68. In addition, the CLICK systems can be installed from the front without having to counter the cable entry from the rear (installation by clicking into place). The installation type can be determined by the users themselves, in line with the required IP protection class. Retrofitting or service work can be done easily at any time with the new CLICK system.  
Depending on the type of installation, the KEL-DPZ-CLICK has got the certified protection classes IP65, IP66 and IP68, RINA, HL3, ECOLAB and many more.  
Free samples are available directly from the manufacturer.  
<https://www.icotek.com/en-us/products/cable-entry-plates/kel-dpz-click>

*  
Image: icotek KEL-DPZ-CLICK, front and back side*

**icotek Corp.   
North American Headquarters**  
Press contact  
Stephan Buchner  
130 S Jefferson St Suite LL150  
Chicago, IL 60661, USA  
[www.icotek.com](http://www.icotek.com)  
[info@icotek-usa.com](mailto:info@icotek-usa.com)  
[s.buchner@icotek.com](mailto:s.buchner@icotek.com)  
2021-04