**Press Release** **icotek KTMBS (1056/1251 digits)**

**New Split Multi-Range Grommets from icotek**


With the KTMBS grommet series, icotek is proud to announce a NEW slotted, multi-range grommet for use with our entry frame and cable gland series. Thanks to its split design, the new KTMBS series is used for the routing of pre-assembled and non-assembled cables. Twelve different grommet sizes are available. The entire grommet series covers a clamping range of 4 to 29 mm of cable diameter.

In addition, the split side of the grommet is perforated with an innovative wave cut. This corrugated cut and the flexible membrane of the KTMBS grommet enable the increased sealing of the routed cables.

The cable diameter can vary up to 3 mm due to a special membrane. The flexible grommet offers the engineer a lot of leeway on site: If the exact cable diameter is not known before installation, the installer can react quickly and flexibly with the KTMBS multi-area grommet from icotek.

The KTMBS is made of elastomer. The KTMBS series is silicone and halogen free. The operating temperature range is -40C° to 100°C. The new split multi-range grommet is now available.

Samples and certificates can be obtained from the manufacturer.

https://www.icotek.com/en-us/products/cable-grommets/ktmbs 

*Image: icotek KTMBS 12-15*

**icotek Corp.   
North American Headquarters**  
Press contact  
Stephan Buchner  
130 S Jefferson St Suite LL150  
Chicago, IL 60661, USA  
[www.icotek.com](http://www.icotek.com)  
[info@icotek-usa.com](mailto:info@icotek-usa.com)  
[s.buchner@icotek.com](mailto:s.buchner@icotek.com)  
2022-03