**Press release KT-SC (984/1168 digits)**

**icotek Grommet with Staged Membrane Rings**

icotek presents its new cable grommet KT-SC with peelable membrane rings. The new cable grommet KT-SC has removable rings with graduated sealing areas.  
The new grommet KT-SC is based on the grommet size "KT large" from icotek. It enables the routing and sealing of cables and hoses with diameters from 5 to 28 mm. The single membrane rings can be peeled away according to the diameter of the routed cable or hose. All you have to do is pierce a small hole between the rings. Afterwards the corresponding ring can be removed. The rings are marked with the letters A to F. This marking shows the corresponding diameter of the inserted cable. The KT-SC can be integrated into all divisible cable entry frames (KEL, KEL-U, KEL-ER, KVT and KEL-FG) which accommodate large KT cable grommets.  
The KT-SC is made of elastomer, achieves IP54 class and is suitable for a temperature range between - 40 ° C to + 100 ° C. The cable grommet is halogen and silicone free.  
Free samples and further information are available directly from the manufacturer.

<https://www.icotek.com/en-uk/product-catalogue/cable-entry-systems/cable-grommets/kt-sc/>

****

**icotek Corp.   
North American Headquarters**  
Press contact  
Stephan Buchner  
130 S Jefferson St Suite LL150  
Chicago, IL 60661, USA  
[www.icotek.com](http://www.icotek.com)  
[info@icotek-usa.com](mailto:info@icotek-usa.com)  
[s.buchner@icotek.com](mailto:s.buchner@icotek.com)  
2020-01