**Press release** **icotek FP-AX-BES-U (654/764 digits)**

**Two-part flange plates FP-AX-BES-U from icotek**

icotek offers its newest flange plates FP-AX-BES-U. The two-part flange plates are designed for RITTAL enclosures type AX.

The FP-AX-BES-U each have two brush strips which are arranged opposite each other and with different filling heights (1 x 35 mm and 1 x 50 mm).

The overlapping of the brush strips increases the tightness and prevent dirt from entering the housing.

The principle of the flange plates FP-AX-BES-U is tried and tested and impresses with its simple assembly.

The ready-for-installation flange plate is made of sheet steel and is powder-coated. The approved temperature range is -20°C to + 90°C.

The FP-AX-BES-U is halogen and silicone free.

<https://www.icotek.com/en/products/enclosure-accessories/fp-bes-u>



*Image: FP-AX-BES-U*



*Image: FP-AX-BES-U Application*

**icotek GmbH**Press contact  
Stephan Buchner  
Bischof-von-Lipp-Str.1, 73569 Eschach  
[www.icotek.com](http://www.icotek.com)  
[s.buchner@icotek.com](mailto:s.buchner@icotek.com)  
September 2021