**Press release** **icotek KTMBS (1063/1252 digits)**

**New split multi-range grommets from icotek**


With the KTMBS series, icotek presents their new splitted multi-range grommets for its cable entry frames and cable glands. Thanks to its split design, the new KTMBS series is used for the routing of pre-assembled and non-assembled cables. Twelve different grommet sizes are available. The entire grommet series covers a clamping range from 4 to 29 mm.

In addition, the split side of the grommet is perforated with an innovative wave cut. This corrugated cut and the flexible membrane of the KTMBS grommet enable the increased sealing of the routed cables.

The cable diameter can vary up to 3 mm due to a special membrane. The flexible grommet offers the engineer a lot of leeway on site: If the exact cable diameter is not known before installation, the fitter can react quickly and flexibly with the KTMBS multi-area grommet from icotek.

The KTMBS consists of elastomer. The KTMBS series is silicone and halogen free. The permissible temperature range is -40C° to 100°C. The new split multi-range grommet is now available.

Samples and certificates can be obtained from the manufacturer.

https://www.icotek.com/en/products/cable-grommets/ktmbs

*Image: icotek KTMBS 12-15*

**icotek GmbH**Press contact  
Stephan Buchner  
Bischof-von-Lipp-Str.1, 73569 Eschach  
[www.icotek.com](http://www.icotek.com)  
[s.buchner@icotek.com](mailto:s.buchner@icotek.com)  
March 2022