**Press release KEL-DPU-OD (1914/2234 characters)**

**New cable entry plate KEL-DPU-OD: Reliable protection under extreme conditions**

With the new cable entry plate KEL-DPU-OD, icotek presents an innovative solution for applications that are permanently exposed to strong UV radiation, weathering, and temperature fluctuations. The robust, snap-in entry plate impresses with its high material resistance, extended service life, and versatile indoor and outdoor applications.

Thanks to its F1 listing in accordance with UL 746C, the KEL-DPU-OD meets the highest requirements for UV and weather resistance. This makes it particularly suitable for photovoltaic systems, energy and environmental technology, and industrial outdoor installations. Its approvals in accordance with UL 6703, UL 6703A, UL 3703, and UL 1703 underline its high quality and safety standards.

“With the KEL-DPU-OD, we are responding to the growing demand for durable cable management solutions for outdoor applications. It offers users maximum safety, tightness, and ease of installation—even under extreme conditions,” explains [David Wetzel, Product Manager, icotek].

The cable entry plate allows numerous cables with diameters from 3.2 to 20.5 mm to be routed in the smallest of spaces and ensures double sealing with IP66/IP68 and UL Type 4X. Its snap-in design and screw mounting option allow for flexible and quick installation. Pierced membranes can be resealed with ST-B plugs.

A special advantage: Optionally available threaded bushings allow installation from the inside of the enclosure – effective protection against vandalism and unauthorized access.

With its high packing density, excellent strain relief, and outstanding material quality, the KEL-DPU-OD offers an economical and durable solution for demanding applications in industrial environments.

Brief profile

• Product: KEL-DPU-OD – Cable entry plate for extreme conditions

• Protection class: IP66 / IP68 / UL Type 4X

• Approvals: UL 6703, UL 6703A, UL 3703, UL 1703, F1 listed (UL 746C)

• Cable diameter: 3.2 – 20.5 mm

• Mounting: Snap-in or screw mounting

• Special features: UV and weather resistant, vandal-proof version available, reusable membranes

<https://www.icotek.com/en/products/cable-entry-plates/kel-dpu-od>

Ein Bild, das Elektrische Leitungen, Verbindungsstück, Stromversorgung, Schrumpfschlauch enthält.

KI-generierte Inhalte können fehlerhaft sein.

*Image: KEL-DPU-OD 24|14*

**icotek GmbH & Co. KG**Press contact  
Stephan Buchner  
Bischof-von-Lipp-Str.1, 73569 Eschach  
[www.icotek.com](http://www.icotek.com)  
[s.buchner@icotek.com](mailto:s.buchner@icotek.com)  
November 2025