**Press release** **icotek KEL-DPZ 10 (1093/1293 digits)**

**New Cable Entry Plates KEL-DPZ 10**

icotek is expanding its range of tool-free mountable cable entry plates with the compact KEL-DPZ 10.

With the new size, up to 26 cables are inserted into a very small space and sealed twice in accordance with IP65 / IP66 / UL Type 12. At the same time, cables are strain-relieved. The diameter of the routed cables can vary from 3.2 to 12 mm. The KEL-DPZ product series are free of dirt-collecting recesses due to the hygienic design.

The KEL-DPZ 10 fits on cut-outs that are standardized for 10-pin heavy-duty connectors. It is a cost-effective, space-saving and quick-to-install alternative to conventional cable glands and has a high packing density.

The KEL-DPZ cable entry plates are ideally suited for the routing of cables without connectors. The assembly with electrical and pneumatic hoses can be done quick and easy: Simply make a small hole in the thin membrane and push the cables through. ST-B Plugs can be used for sealing pierced membranes if cables have been removed.

The certification of the protection classes IP65 / IP66 took place according to DIN EN 60529: 2000-09.

The new sizes are available from now on. Free samples can be obtained directly from the manufacturer.

<https://icotek.com/en-us/products/cable-entry-plates/kel-dpz>



*Image: KEL-DPZ 10*

**icotek Corp.   
North American Headquarters**  
Press contact  
Stephan Buchner  
130 S Jefferson St Suite LL150  
Chicago, IL 60661, USA  
[www.icotek.com](http://www.icotek.com)  
[info@icotek-usa.com](mailto:info@icotek-usa.com)  
[s.buchner@icotek.com](mailto:s.buchner@icotek.com)  
2021-12