**Press release LFC (823/974 digits)**

**New EMC Shield Clamps For Use On C-rails**


The new EMC shield clamps LFC-MSKL and LFC-SKL are used for mounting with clamps on C-rails.

The LFC contacts the cable shield directly on the C-rail. The existing cable clamp can still be used. The strain relief takes place via the cable sheath, since the shield connection is not designed for mechanical loads. The large shield contact and strain relief are correctly separated. icotek’s shield clamps type SKL / MSKL are used wherever the shield of individual cables has to be connected to the ground potential.

The tool-free, space-saving assembly and the high vibration resistance of the EMC shield clamps are of great advantage. The LFC also has a large clamping range of 3 - 30 mm and offers great flexibility. The LFC is suitable for mounting on all common C-rails with an opening dimension of 16-17 mm.

The new shield clamps are now available from the manufacturer.

<https://www.icotek.com/us/product-catalog/emc-cable-clamps/lfc/>

****

**icotek Corp.   
North American Headquarters**  
Press contact  
Stephan Buchner  
130 S Jefferson St Suite LL150  
Chicago, IL 60661, USA  
[www.icotek.com](http://www.icotek.com)  
[info@icotek-usa.com](mailto:info@icotek-usa.com)  
[s.buchner@icotek.com](mailto:s.buchner@icotek.com)  
2020-04