**Press release** **icotek KEL-DPZ 10 (1090/1290 digits)**

**New cable entry plates KEL-DPZ 10**

icotek is expanding its range of tool-free mountable cable entry plates with the compact KEL-DPZ 10.

With the new size, up to 26 cables are inserted into a very small space and sealed twice in accordance with IP65 / IP66 / UL Type 12. At the same time, cables are strain-relieved. The diameter of the routed cables can vary from 3.2 to 12 mm. The KEL-DPZ product series are free of dirt-collecting recesses due to the hygienic design.

The KEL-DPZ 10 fits on cut-outs that are standardized for 10-pin heavy-duty connectors. It is a cost-effective, space-saving and quick-to-install alternative to conventional cable glands and has a high packing density.

The KEL-DPZ cable entry plates are ideally suited for the routing of cables without connectors. The assembly with electrical and pneumatic hoses can be done quick and easy: Simply make a small hole in the thin membrane and push the cables through. ST-B Plugs can be used for sealing pierced membranes if cables have been removed.

The certification of the protection classes IP65 / IP66 took place according to DIN EN 60529: 2000-09.

The new sizes are available from now on. Free samples can be obtained directly from the manufacturer.

https://icotek.com/en/products/cable-entry-plates/kel-dpz



*Image: KEL-DPZ 10*

**icotek GmbH**Press contact  
Stephan Buchner  
Bischof-von-Lipp-Str.1, 73569 Eschach  
[www.icotek.com](http://www.icotek.com)  
[s.buchner@icotek.com](mailto:s.buchner@icotek.com)  
December 2021